**Real-Time, Non-Contacting Position Tracking of Medical Devices and Surgical Tools through the Analysis of Magnetic Field disturbances**

Mohammad Odeh1

Edward Daniel Nichols1

Fluvio Lobo1

Jack Stubbs1

Institute for Simulation and Training,

University of Central Florida1

RED, BOLD, ITALICS\* Need to be reviewed, double-checked for accuracy, or updated as the system progresses.

# 1 Background

As the demand for increasingly advanced invasive medical procedures rises with the average age of the population, it also becomes increasingly compelling to facilitate and extend the spatial awareness and dexterity of surgeons, both human and robotic. One may accomplish this by tracking an object digitally and representing its motion in a close virtual representation of the area around the incision, such as through an augmented reality platform. Several groups across a diverse range of academia and industry have competed to develop better and better methods of digitally tracking objects ***[CITATION]***. In the entertainment industry in particular, object tracking is a fundamental way of bringing life-like motion to an object represented in virtual space. The generally accepted approach is to use large, complicated, and expensive computer vision (CV) systems to yield real-time tracking ***[CITATION]***. However, this approach is not suited for medical applications; CV is limited by a strict field of view. Accurately tracking surgical instruments inside of organic tissues must then be done another way.

Of the methods investigated by others ***[CITATION]***, none are as applicable in a medical context as magnetic field sensing. Human tissues are permeable to magnetic flux, and magnetic fields are well characterized. Upon this motivation, we have constructed an inexpensive device from off-the-shelf parts that enables the tracking of a permanent magnet on a ***contoured surface*** to serve as a foundation for future work in this field.

# 2 Methods

## 2.1 Theoretical background

Electromagnetic fields are characterized by fundamental principles. Given a classic magnetic dipole centered at the origin, its magnetic induction can be expressed as:

|  |  |
| --- | --- |
|  | (1) |

Whereby the relationship is dependent on the orientation of the magnet and the strength of its magnetic moment vector, given by , as well as the location of the arbitrary point of interest with respect to the center of the magnet, represented by vector . Equation (1) can be modified to express the strength of the magnetic field **,** which is what an observing magnetometer normal to the level surface of the magnetic field would perceive; which may further be broken into a more convenient polar component form, given the intrinsic rotational symmetry of isofield lines about .

Based on the work of Chen *et al* ***[FINEXUS CITATION]***, expressing the location of the center of a magnet with respect to the magnetic field vectors observed by three sensors in predefined relative positions satisfies a system of equations when the magnet is in a fixed orientation ***along the sensor’s x-axis***:

|  |  |
| --- | --- |
|  | (2) |
|  | (3) |
|  | (4) |

Whereby, represents a sensor in the array, is the distance to the center of the magnet for the sensor, is the relative offset from a designated origin with respect to the sensor, represents the angle made by the north pole of the magnet and the radial component of, and K represents a constant that encompasses the magnitude of the dipole moment, magnetic permeability of free space, and the relative permeability of the magnet’s material.

However, one must maintain certain minimum assumptions for a solution to converge in a numerical solver.

1. An origin must be defined with respect to the relative fixed positions and orientations of the sensors.
2. The constant value of the magnetic field strength coefficient K of an arbitrary magnet has been closely approximated, or is otherwise known.
3. The constant magnetic field source of perceivable threshold exists within range of at least three sensors in the sensor array.

In addition, to refine accuracy, certain physical restrictions facilitate these conditions.

1. Ambient magnetic fields must be mitigated; or the signal must be otherwise overcome.
2. The magnet’s form factor is minimized to yield closer adherence to presupposed principles.

To begin achieving these conditions, we designate the sensor in the bottom left corner of our array to be the origin. All sensors’ axis in the array are aligned with each other.

## 2.2 Empirical Approximation of K

|  |  |
| --- | --- |
|  | (5) |

Equation (5) is derived from Eqns. (3) and (4) if motion occurs along a single axis, namely, *x***.**Empirically approximating the value of K for an arbitrary dipole magnet can then be done procedurally. A proof of concept was completed by hand. We have done this precisely using a custom CNC machine. As follows:

1. The magnet is placed at a particular distance away from sensor *i* such that (*x*, y = 0, z = 0).
2. A sample of K is computed from for sensor *i*.
3. The magnet is moved to = (, y = 0, z = 0).
4. Another sample of K is computed from.
5. The process is repeated a few iterations for various values of, and for each sensor.
6. An approximated result of K yields from averaging the sampled points.

## 2.2 Sensor Array

**[INSERT PICTURE OF ARRAY]**

The first prototype consisted of a pair of IMUs across from each other calculating the distance to the magnet and triangulating a location from there. Additional sensors were added to enable ***limited*** 3D tracking and extend the range. The array is ***finally comprised of six*** *Sparkfun LSM9DS1 IMU* *breakouts* arranged in a circular pattern around a central area. They are switched to by a *Sparkfun 74HC4051 8-channel* *multiplexer* *breakout*, and data is driven through the Arduino compatible *PJRC Teensy v3.2* via I2C. This information is then lightly manipulated and output, line by line, through Serial Bus to a capable Python script on a PC.

Sensor readings are taken by the IMUs every ***[PERIOD]***, yielding the XYZ components of with respect to the sensor orientation. Geomagnetism is partially accounted for with the IMUs’ built-in function given a local declination. To mitigate the effect of remaining ambient magnetic fields, sensor readings are averaged over 50 readings upon reset and the result is subtracted from later readings for each sensor, respectively. Drifting is observed to be minimal, yet further mitigation is left as future work. Readings henceforth start at ±20 milliGauss and range to ±16 Gauss, according to the built-in 16-bit analog to digital converter in the IMU chip. This information for each sensor is output by the *Teensy* to the PC, where it is split and sorted by the Python script.

## 2.3 Position Tracking Algorithm

Each sensor allows the script to assemble one possible input equation according to Eqns. (2), (3) and (4) for a total of six coupled equations. As can be observed, the constructed system of equations is non-linear and has no analytical solution, thus the need for a numerical technique to aid in the computation of the magnet’s position arises. Computation begins after the script has assembled the nonlinear system of equations and chosen the three rendered from the sensors calculated to have the largest respective to pass to a Levenberg-Marquardt algorithm (LMA) powered by the versatile *SciPy* module. The reason that only three equations are being considered during the computation process stems from the fact that *SciPy*’s implementation of the LMA lacks support for overdetermined systems of equations.

LMA was chosen for its robustness and speed of convergence. Its accessibility within *SciPy*, notwithstanding. Furthermore, since LMA combines Newton-Raphson’s algorithm and the Steepest Descent method, it converges to a solution even if the initial guess is far off the mark. Yet, to reduce computation time, the script performs a dynamic search of the possible initial guesses by determining the possible location of the magnet in accordance to which three sensors are reading the highest magnetic field. The initial guess is then determined as the centroid of the triangle formed by the three sensors and is fed into the LMA.

A permanent magnet of ***[DIMENSIONS]*** is chosen as the source and assumed to have an ideal magnetic dipole field at long-distance.

Further optimization is required, especially and including the mitigation of ambient fields, the sampling rate, computation time, arbitrary orientations of the magnet, and ***[LIVE PLOT REFRESH RATE?].*** We have identified these issues and leave their resolution to future work.

# 3 Results

The results are;

1. Sensor array for real-time, non-contacting tracking of an object along a plane
2. Sensor array for real-time, non-contacting tracking of an object in space (3D)
3. An robust algorithm for the real-time, non0-contacting tracking of an object in space (3)

The robustness of our sensor arrays (devices) and analysis software was evaluated in terms of;

* Examples of data plot
* Speed of the data
* Accuracy and precision
* Discuss permeability of materials to magnetic flux

# 4 Interpretation

The Interpretation section provides an interpretation of the results and conclusions of the study.

* Limitations of the approach
  + No visualization of the orientation of the magnet, yet.
  + Only one magnetic point at a time.
* Other calibration considerations
* How to improve!
  + Optimize software.
  + Improve data sampling rate.
  + Redress fundamental principles; higher abstraction models.

# References

References follow ASME style, described in See the “Writing a Technical Paper or Brief” section, under Guidelines at the ASME Journal Tool Author Help (<http://tinyurl.com/43chze9>)

* All references need to be complete citations with ALL authors listed (As per style et al. is not allowed in the reference list.), starting page number and ending page number, doi if available, etc. **examples:**
  + Brigitte, M., Max, S., Juergen, H., Peter, M., Bernd, K., & Eckhart Georg, H. (1999). Disposable-sheath, flexible gastroscope system versus standard gastroscopes: a prospective, randomized trial. Gastrointestinal Endoscopy, 50461-467. doi:10.1016/S0016-5107(99)70066-0
  + Ma, J. and Kim, H. M., 2014, “Continuous Preference Trend Mining for Optimal Product Design With Multiple Profit Cycles,” J. Mech. Des., 136(6), 061002, doi: 10.1115/1.4026937

[FORMATTING NOTES]

* Entire paper is two to four pages. Top and bottom page margins are one inch so that total text height is 9 inches. There are two columns, with the title area being in the first column. Columns are 3.125 inches wide and the spacing between the two columns is 0.25 inches for a total text width of 6.5 inches. Columns are justified left and right.
* Font for title, headers, body text is Times. Body text is 9 point. Title is 14-point bold. Authors and affiliation are 11-point with author names in bold..
* New paragraphs are indented by 0.2 inches, no blank line between paragraphs.
* There are no page numbers.
* Provide definition for all acronyms. Example: deep brain stimulation (DBS)
* When in doubt, look at an article in an ASME journal.
* See the “Writing a Technical Paper or Brief” section, under Guidelines at the ASME Journal Tool Author Help ([**http://tinyurl.com/43chze9**](http://tinyurl.com/43chze9)) for handling mathematics, equations, figures and tables.